

PROJECT REPORT

POINT OF SALE WITH INTERNET OF THINGS



November 27, 2020

AI KAIROS

* Problem Definition

The problem we are trying to solve here is mainly related to advertising with a secondary application of POS.

1. Companies usually pay the vendors/salesmen a hefty price just to advertise their products and it usually happens that the banners are just made and not used etc. or are either placed in positions not visible to customers.
2. Sometimes the customer just considers the product and doesn’t buy it, this can be used by companies to test different strategies like what changes drive the crowd based on different entities/constraints, etc.

* The originality of the work/Plagiarism declaration

It is a part of my internship at AI Kairos and I am trying to deliver the best from my side. And as for plagiarism, it is implemented by very few companies like AWM & Amazon but the source code and procedures are completely privatized for the betterment of the company.

* Project description

The purpose of the project is to make use of IOT sensors to compare the data with POS or to ensure the proper placement of advertisement banner preferably in lime light areas or to determine if a product is in the customers consideration funnel.

* + Project Overview
* It is a requirement/recommendation of one of the tie ups of AI Kairos, and their main intent is to make the surveys more meaningful which can be accomplished from the data obtained from this project.
  + Project Organization
* Mrs Swati is the project head and handles the complete project along with Milind Sir.
  + Opportunity Statement
* This project started with the aim of tracking POS style functionality and is still aimed at doing so, but due to technical incapability, it was decided to carry out in chunks.
  + Impact Statement
* The project will help resolving many issues of which two are described in the problem definition, and also has a potential to predict inventory with help of ML.
  + Project Objectives
* A minimal dashboard that can display various graphs based on the recorded data.
  + Project Scope
* The main scope is to gain minimum functionality that is to determine whether a person is standing in front of the shelf or advertisement banner or not, and then further with sensors on every shelf observer if the person picked up and again discarded the product.
  + Constraints and Assumptions

[currently none – to be introduced in next iteration with UI development].

* Details of development –


## Product Perspective

A self-contained, standalone product mainly targeted to use IOT as to integrate and improve upon already existing local POS systems

* + Technologies
    - Internet of Things
      * PIR Sensor
      * ESP8266
    - Python
      * Visual Studio Code
    - Point of Sales (to be decided)
    - UI (either pyqt5 or django)
  + Data [planned for next iteration]
    - Still a slight vision on how it will work is, the way how HC501 sends a high signal when it senses motion, we will convert the high signal to 1 and low to 0 along with time straps of high signal and use the data accordingly.
  + Theory


## **Working of PIR sensor**

PIR motion sensors consist of two main parts: a **pyroelectric sensing element** and a **fresnel lens**. The pyroelectric sensing element can detect infrared radiation. All objects with a temperature above absolute zero (0 Kelvin / -273.15 °C) emit heat energy in the form of infrared radiation, including human bodies.




A pyroelectric sensor has two rectangular slots in it made of a material that allows the infrared radiation to pass. Behind these, there are two separate infrared sensor electrodes, one responsible for producing a positive output and the other a negative output. The reason for that is that we are looking for a change in IR levels and not ambient IR levels. The two electrodes are wired up so that they cancel each other out. If one half sees more or less IR radiation than the other, the output will swing high or low.

The on-board signal processing IC processes this signal and turns the output pin of the sensor HIGH or LOW accordingly.



The white dome in front of the sensing element is a fresnel lens. This lens focuses the infrared radiation onto the sensor.



## **HC-SR501 PIR Motion Sensor**

The HC-SR501 PIR motion sensor is built around the BISS0001 Micro Power PIR Motion Detector IC. This IC is specifically developed to process the signal from PIR motion sensors.

If you remove the fresnel lens, you will see the RE200B pyroelectric sensing element. On the PCB you can also find a built-in voltage regulator. This means you can power the board with a large DC voltage range, typically 5 V is used.


The specifications of the HC-SR501 are given in the table below, note that there might be small differences between manufacturers.

### HC-SR501 Specifications

|  |  |
| --- | --- |
| Operating voltage | 4.5 – 20 V |
| Quiescent current | 50 μA |
| Level output | HIGH 3.3 V / LOW 0 V |
| Trigger | L single trigger / H repeating trigger |
| Delay time | 3 – 300 s |
| Blocking time | 2.5 s (default) |
| Trigger | L single trigger / H repeating trigger |
| Measuring range | 3 – 7 m maximum |
| Measuring angle | < 110° cone angle |
| PCB dimensions | 32.5 x 24 mm |
| Mounting holes | 2 mm, 28.5 mm spacing |
| Fresnel lens dimensions | 15 mm x 23 mm diameter |
| Operating temperature | -15 – 70 °C |

### Adjusting the HC-SR501

On the back of the board you will find two potentiometers and a jumper, which you can use to adjust several parameters:



#### Sensitivity (range) adjustment

The HC-SR501 has a maximum sensing distance (detection range) of 7 meters. You can adjust the sensing distance by rotating the sensitivity potentiometer CW or CCW (see picture above). Rotating the potentiometer clockwise increases the sensing distance to a maximum of 7 meters. Rotating it counter-clockwise decreases the sensing distance to a minimum of 3 meters.

#### Time-delay adjustment (Tx)


This potentiometer can be used to adjust the time that the output stays HIGH for after motion is detected. At a minimum, the delay is 3 seconds and at a maximum, it is 300 seconds or 5 minutes. Turn the potentiometer clockwise to increase the delay and counter-clockwise to decrease the delay.

#### Trigger selection jumper

The (yellow) jumper can be used to select one of the two trigger modes. It can be set to either **L** (single trigger) or **H** (repeating trigger):

* **Single trigger** – The output will turn HIGH as soon as motion is detected. It will stay HIGH for the time set by the potentiometer. Any movement during this period is not processed and does not restart the timer.
* **Repeating trigger** – Every time motion is detected, the delay timer is restarted.

The difference between the single and repeating trigger mode is shown in the figure below.




Difference between single and repeating trigger mode. The arrows indicate the set delay-time.


* + Diagrams [added in respective sections]
  + Charts

\*\*(expected to change with change in working or requirement or in rare cases constraints)


\*Remaining diagrams will be added with the implementation of a UI. (which is currently a future scope for next semester)

UML Diagrams


* Structural Diagrams
  + Class Diagram
  + Component Diagram




* + Deployment Diagram




* + Package Diagram
  + Composite Structure Diagram
  + Object Diagram
  + Profile Diagram
* Behavioral Diagram
  + Activity Diagram




* + Use case Diagram




* + State Machine Diagram

**

* + Interaction/Communication Diagram



* + Sequence Diagram



* + Interaction Overview Diagram
  + Timing Diagram
* Database design

[not necessarily required]/ (future scope along with UI)

\*\*in case if applicable will be using the technology compatible with the host server.

* Applications –
  + Methods
    - With Raspberrypi – useful for advertisement boards.
      * Advantages

1. All in one functionality
2. Extremely flexible
3. Future Proof
4. Ample of resources
5. No requirement of extensions
6. Seamless upgradation
7. No skill required
8. Can also handle the sync functionality on its own
   * + - Limitations
         1. Expensive
         2. Power requirement is high
     + With Arduino – good for custom requirement
       - Advantages
9. Comparatively affordable
10. Moderate power requirement
    * + - Limitations
          1. Requires different modules and extensions to work
          2. Skilled person is required to handle
          3. Requires external source for computation
      + With bare relay – bulk installation for example shelf
        - Advantages
11. Very Cheap
12. Semi-skilled labour required
13. Minimal power requirement
    * + - Limitations
14. Requires external source for computation
15. No scope for future upgrades

* Project Code & Snapshots/Output
  + Methods
    - Through Raspberrypi

Code:

import RPi.GPIO as GPIO #Import GPIO library

import time #Import time library

GPIO.setmode(GPIO.BOARD) #Set GPIO pin numbering

pir = 26 #Associate pin 26 to pir

GPIO.setup(pir, GPIO.IN) #Set pin as GPIO in

print "Waiting for sensor to settle"

time.sleep(2) #Waiting 2 seconds for the sensor to initiate

print "Detecting motion"


while True:

if GPIO.input(pir): #Check whether pir is HIGH

print "Motion Detected!"

time.sleep(2) #D1- Delay to avoid multiple detection

time.sleep(0.1) #While loop delay should be less than detection(hardware) delay



* + - With Arduino

Code:

/\*PIR HCSR501 \*/

int ledPin = 13; // LED

int pirPin = 2; // PIR Out pin

int pirStat = 0; // PIR status

void setup() {

pinMode(ledPin, OUTPUT);

pinMode(pirPin, INPUT);

Serial.begin(9600);

}

void loop(){

pirStat = digitalRead(pirPin);

if (pirStat == HIGH) { // if motion detected

digitalWrite(ledPin, HIGH); // turn LED ON

Serial.println("Hey I got you!!!");


}

else {

digitalWrite(ledPin, LOW); // turn LED OFF if we have no motion

}

}



* + - Bare Relay Method [WIP]

Code:

#include <ESP8266WiFi.h>

#include <Base64.h>

//AP definitions

#define AP\_SSID "your AP SSID"

#define AP\_PASSWORD "your AP password"

// EasyIoT server definitions

#define EIOT\_USERNAME "admin"

#define EIOT\_PASSWORD "test"

#define EIOT\_IP\_ADDRESS "192.168.1.5"

#define EIOT\_PORT 80

#define EIOT\_NODE "N8S0"

#define INPUT\_PIN 2

#define USER\_PWD\_LEN 40

char unameenc[USER\_PWD\_LEN];

bool oldInputState;

void setup() {

Serial.begin(115200);

pinMode(INPUT\_PIN, INPUT);

wifiConnect();

char uname[USER\_PWD\_LEN];

String str = String(EIOT\_USERNAME)+":"+String(EIOT\_PASSWORD);

str.toCharArray(uname, USER\_PWD\_LEN);

memset(unameenc,0,sizeof(unameenc));

base64\_encode(unameenc, uname, strlen(uname));

oldInputState = !digitalRead(INPUT\_PIN);

}

void loop() {

int inputState = digitalRead(INPUT\_PIN);;

if (inputState != oldInputState)

{

sendInputState(inputState);

oldInputState = inputState;

}

}

void wifiConnect()

{

Serial.print("Connecting to AP");

WiFi.begin(AP\_SSID, AP\_PASSWORD);

while (WiFi.status() != WL\_CONNECTED) {

delay(1000);

Serial.print(".");

}

Serial.println("");

Serial.println("WiFi connected");

}

void sendInputState(bool inputState)

{

WiFiClient client;

while(!client.connect(EIOT\_IP\_ADDRESS, EIOT\_PORT)) {

Serial.println("connection failed");

wifiConnect();

}

String url = "";

String command = "";

if (inputState)

command = "ControlOn";

else

command = "ControlOff";

url = "/Api/EasyIoT/Control/Module/Virtual/"+ String(EIOT\_NODE) + "/"+command; // generate EasIoT server node URL

Serial.print("POST data to URL: ");

Serial.println(url);

client.print(String("POST ") + url + " HTTP/1.1\r\n" +

"Host: " + String(EIOT\_IP\_ADDRESS) + "\r\n" +

"Connection: close\r\n" +

"Authorization: Basic " + unameenc + " \r\n" +

"Content-Length: 0\r\n" +

"\r\n");

delay(100);

while(client.available()){

String line = client.readStringUntil('\r');


Serial.print(line);

}

Serial.println();

Serial.println("Connection closed");

}



* + Functions

Clients:

* Create and own multiple stores to display and sell products
* Create, read, update, and delete both local and online inventories
* Monitor Sales online through the web application

Customers:

* Create, read, update, and delete a personal, shopping cart
* View, purchase, and pay for items electronically through various mediums

Windows Syncing Service

* Resolves conflicts between online and offline inventories
* Provides transaction data to the client
* Provides real time statistics of sold products(sales) to the client
* Receives and transmits inventory data to and from each local client and the server
* Future scope
  + Make a user interface for the CLI.
  + Integrate sync APIs.
  + etc
* References

1. <https://www.makerguides.com/hc-sr501-arduino-tutorial/>
2. <https://iot-playground.com/blog/2-uncategorised/42-esp8266-wifi-pir-motion-sensor-arduino-ide>
3. <https://www.instructables.com/How-to-Use-PIR-Motion-SensorHC-SR501with-an-Arduin/>
4. <https://electrosome.com/pir-motion-sensor-hc-sr501-raspberry-pi/>

For further tracking my project follow this GitHub link:

[**https://github.com/gkKshitij/POS-recording-with-IOT**](https://github.com/gkKshitij/POS-recording-with-IOT)

* Glossary

**POS:** An acronym for Point of Sales, which is the place where a transaction occurs in exchange for goods or services

**PHP:** An open source server­-side scripting language designed for Web development to produce dynamic Web pages

**Client:** An owner and operator of a single instance of the installation

**Customer:** One of the users of a client’s service & buyer of the products.

**Administrator:** A person who manages the servers and products

.  
**GUI:** An acronym for graphical user interface, it is a type of user interface that allows users to  
interact with electronic devices using images rather than text commands

**UI:** An acronym for user interface. A UI is the space designed for interaction between humans and machines.

**MySQL:** The world's most used open source relational database management system

**Intuit:** An American software company that develops financial and tax preparation software and related services for small businesses, accountants and individuals

**Sync:** A term for the process for retrieving data, resolving conflict in the data, and sending the data back

**OS:** Operating System. The main software that controls interactions from the hardware of the  
computer to the software that runs on the computer

**API:** An acronym for application programming interface. An API is a protocol intended to be used as an interface by software components to communicate with each other

**ML: Machine Learning**

**CLI: Command line interface**